|  |
| --- |
| **SD-27 SIRIO DIPOLE** ANTENA DIRECTIVA RIGIDA 27 MHZType: 1/2 wave Dipole Frequency range: 26-29 MHz Impedance: 50 Ohms unbalanced Radiation (H-plane): Horizontal mounting: Directional Vertical mounting: Omnidirectional Polarization: horizontal SD 27 SIRIO DIPOLE |

|  |
| --- |
|  |
|  |
|  |
|  |

|  |  |
| --- | --- |
|  |  |
|

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  | http://www.locuradigital.com/templates/jcc/images/referencia/redonda.jpgCARACTERÍSTICAS  |  |
|  |  |  |

 |

|  |
| --- |
|  Gain: 0 dBd, 2.15 dBi  Bandwidth at S.W.R. 2:1: 3750 KHz  S.W.R. at res. freq.: = 1.1:1  Max. power:1000 Watts (CW) Continuous, 3000 Watts (CW) short time  Feed system / position: Gamma match / center  Connector: UHF-female  Boom Length: 1400mm Boom Diameter: 33mm Radiator Length (Vertical elements): 5420mm Radiator Diameters: 8-12-16mm Weight (approx): 2.5kg Mounting Mast Diameters: 35/50mm |