|  |
| --- |
| **UBC785XLT UNIDEN COBERTURA DE FRECUENCIAS: 25- 1.300MHz   http://www.locuradigital.com/images_upload/ubc_785xlt_01.jpg**  RECEPTOR SCANNER MOVIL/BASE COBERTURA DE FRECUENCIAS: 25-1.300MHz CANALES DE MEMORIA: 1000 BANCOS DE BUSQUEDA: 10 MODOS DE RECEPCION: AM, FM & WFM SALTOS PROGRAMABLES: 5/6.25/8.33/10/12.5/25/50/100 kHz DISPLAY ALFANUMERICO (2 LINEAS, 16 CARACTERES) DECODIFICACION TRUNKING: Motorola, EDACS, LTR DECODIFICA:CTCSS/DCS   MODOS AM/ FM(estrecha y ancha) ·   HIPERBUSQUEDA·   10 BANCOS DE RASTREO PROGRAMABLES ·   RASTREO DE BANDA,9REA PREPROGRAMADO ·   3 PLANES DE BANDA SELECIONABLES SEGÚN ZONA DE USO·   25 - 1300 MHz(25-512, 806-960,1240-1300) ·   SOPORTE DE SALTOS ESPECIALES 6,25KHZ Y 8,33KHZ(AÉREOS)   -MEMORIAS ALFANUMÉRICAS,DECODIFICACION DE SUBTONOS CTCSS Y DCS.   -PESO 1,3Kg   -DIMENSIONES 177\*69\*168mm   CONTROL REMOTO POR PC CONEXIÓN SERIE RS-232 |

|  |
| --- |
|  |
|  |
|  |
|  |

|  |  |
| --- | --- |
|  |  |
| |  |  |  | | --- | --- | --- | |  |  |  | |  | http://www.locuradigital.com/templates/jcc/images/referencia/redonda.jpgCARACTERÍSTICAS |  | |  |  |  | | |

|  |
| --- |
|  **Wide Frequency Range:** 25 - 512Mhz , 806 - 960Mhz , 1240 - 1300Mhz.   **Frequency steps :** 5 / 6.25 / **8.33** / 10 / 12.5 / 15 / 20 / 25 / 50Khz   **Scan Rate :**100 Channels per sec scan rate   **Speaker :** Built in internal speaker 8 ohm   **Antenna :** Telescopic Antenna Included   **BNC** Type antenna fitting   **Power supply :** AC power supply included   **Size :** 177W x 168D x 69H mm   **Weight :** 1.33Kg |
|  |