|  |
| --- |
| **UBC785XLT UNIDEN COBERTURA DE FRECUENCIAS: 25- 1.300MHzhttp://www.locuradigital.com/images_upload/ubc_785xlt_01.jpg**RECEPTOR SCANNER MOVIL/BASECOBERTURA DE FRECUENCIAS: 25-1.300MHzCANALES DE MEMORIA: 1000BANCOS DE BUSQUEDA: 10MODOS DE RECEPCION: AM, FM & WFMSALTOS PROGRAMABLES: 5/6.25/8.33/10/12.5/25/50/100 kHzDISPLAY ALFANUMERICO (2 LINEAS, 16 CARACTERES)DECODIFICACION TRUNKING: Motorola, EDACS, LTRDECODIFICA:CTCSS/DCS MODOS AM/ FM(estrecha y ancha) ·  HIPERBUSQUEDA·  10 BANCOS DE RASTREO PROGRAMABLES ·  RASTREO DE BANDA,9REA PREPROGRAMADO ·  3 PLANES DE BANDA SELECIONABLES SEGÚN ZONA DE USO·  25 - 1300 MHz(25-512, 806-960,1240-1300) ·  SOPORTE DE SALTOS ESPECIALES 6,25KHZ Y 8,33KHZ(AÉREOS)  -MEMORIAS ALFANUMÉRICAS,DECODIFICACION DE SUBTONOS CTCSS Y DCS.  -PESO 1,3Kg  -DIMENSIONES 177\*69\*168mm  CONTROL REMOTO POR PC CONEXIÓN SERIE RS-232  |

|  |
| --- |
|  |
|   |
|   |
|   |

|  |  |
| --- | --- |
|  |  |
|

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  | http://www.locuradigital.com/templates/jcc/images/referencia/redonda.jpgCARACTERÍSTICAS  |  |
|  |  |  |

 |

|  |
| --- |
|  **Wide Frequency Range:** 25 - 512Mhz , 806 - 960Mhz , 1240 - 1300Mhz.  **Frequency steps :** 5 / 6.25 / **8.33** / 10 / 12.5 / 15 / 20 / 25 / 50Khz  **Scan Rate :**100 Channels per sec scan rate  **Speaker :** Built in internal speaker 8 ohm  **Antenna :** Telescopic Antenna Included  **BNC** Type antenna fitting  **Power supply :** AC power supply included  **Size :** 177W x 168D x 69H mm  **Weight :** 1.33Kg  |
|    |