|  |
| --- |
| **SD-27 SIRIO DIPOLE** ANTENA DIRECTIVA RIGIDA 27 MHZ  Type: 1/2 wave Dipole  Frequency range: 26-29 MHz  Impedance: 50 Ohms unbalanced  Radiation (H-plane):  Horizontal mounting: Directional  Vertical mounting: Omnidirectional  Polarization: horizontal  SD 27 SIRIO DIPOLE |

|  |
| --- |
|  |
|  |
|  |
|  |

|  |  |
| --- | --- |
|  |  |
| |  |  |  | | --- | --- | --- | |  |  |  | |  | http://www.locuradigital.com/templates/jcc/images/referencia/redonda.jpgCARACTERÍSTICAS |  | |  |  |  | | |

|  |
| --- |
|  Gain: 0 dBd, 2.15 dBi   Bandwidth at S.W.R. 2:1: 3750 KHz   S.W.R. at res. freq.: = 1.1:1   Max. power:1000 Watts (CW) Continuous, 3000 Watts (CW) short time   Feed system / position: Gamma match / center   Connector: UHF-female   Boom Length: 1400mm   Boom Diameter: 33mm   Radiator Length (Vertical elements): 5420mm   Radiator Diameters: 8-12-16mm   Weight (approx): 2.5kg   Mounting Mast Diameters: 35/50mm |