> [Products](http://www.luiton.com/htm/product-list.html) > [TRANSCEIVERS](http://www.luiton.com/htm/product-products_type-list.html) > [CB RADIOS](http://www.luiton.com/htm/product-products_type-cb_radios-list.html)

**LT-318 cb radio with CE**



LT-318 Specification

CE Approved

AM/FM CB RADIO

Features:

PC programming

Automatic change power supply 12V/24V

High 8W/Low 4W power switchable

Wide frequency 25-30MHz

Auto scanning

Dual channel standby

Backlight selective (Red,Green,Blue)

ANL function

ASQ

Big LCD display

CH9/CH19 emergency channel

Technical Specifications:

Channel 40 FM (Saw band table)

Frequency range 25.615-30.105 MHz

Operating mode F3E (FM), A3E (AM).

Antenna impedance 50 Ohm

Speaker 8 Ohm3W

Microphone Capacitive

Power 13,6V ± 5%

Dimensions H46xL142xW158 mm

Weight 500G

RECEIVER

Sensitivity in the 12 db S/N0.5µV (AM), 0.25µV (FM)

Selectivitymore than 60dB

Noise range0.25V-500µV

Audio output power 1.5W 8 ohm (10% lost)

Distortion in 1000 µ V5%

Audio frequency response…………………………….…400-2400 Hz

Intermediate frequencyI° 10.695 MHz

II° 455 KHz

Intermodulation anti-interferencemore than 60 dB

TRANSMITTER

RF power output10% HI=10W LO=4W AM/FM

Frequency tolerance……………………………………….005%

Harmonic suppressionmore than 70 dB

Current drainHI=2200 mA LO=900 mA

Modulation mode AM 90% (± 5%)

FM dev. 2.0KHz



