|  |
| --- |
| MFJ976 MFJ Acoplador manual para linea paralela 1500 W 1.8-30 MHz. () |

|  |
| --- |
| The MFJ-976 is a 1500 Watt full legal limit fully balanced antenna tuner. You get superb balance, very wide matching ranges (12-2000 Ohms) and continuous 1.8-30 MHz coverage including all WARC bands! It handles a full 1500 Watts SSB and CW.You can tune any balanced lines including 600 Ohm open wire line, 450/300 Ohm ladder lines, 300/72 Ohm twin lead -- shielded or unshielded. The MFJ-976 also tunes random wires and coax-fed antennas.MFJs fully balanced extremely wide-range T-network gives you simple, fast three knob tuning. No complicated switching between high and low impedance and switching in additional capacitance of L-networks.Four separate 500 pF in two gangs gives you a total of 2000 pF for highly efficient low loss separation on 160 Meters. You get excellent 10 Meter performance because of MFJs low minimum capacitance and exclusive Self-Resonance Killer™ high-Q AirCore™ roller inductor with silver plated contacts.The MFJ-976 1500 Watt Fully Balanced Antenna Tuner has a heavy duty 1:1 current balun that gives you superb balance and stays cool even at 1.5 kW.True active peak reading lighted Cross-Needle SWR/Wattmeter lets you read SWR, true peak or average forward and reflected power all at a glance on 300/3000 Watt ranges. The MFJ-976 unit measures 12W x 6H  inches. |
|   |
|   |
|   |

|  |  |
| --- | --- |
|  |  |
|

|  |  |  |
| --- | --- | --- |
|   |   |   |
|   | http://www.locuradigital.com/templates/jcc/images/referencia/redonda.jpgCARACTERÍSTICAS |   |
|   |   |   |

 |

|  |
| --- |
| MFJ976 MFJ Acoplador manual para linea paralela 1500 W 1.8-30 MHz. |
|   |