|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 124WB CUSHCRAFT | |  |  |  |  | | --- | --- | --- | --- | | 127,00 € | |  |  | | --- | --- | |  | Add to baskethttp://www.radiocenter.es/contents/media/feedback_tick.png | | |

**144-148 MHZ 4 ELEMENTOS, GAIN 10,2DB.**

|  |  |
| --- | --- |
| Model | 124WB |
| 3dB Beamwidth, Degrees E-Plane | 60 |
| 3dB Beamwidth, Degrees H-Plane | 88 |
| Boom Lenght ft.(m) | 4(1.22) |
| Electrical Wavelength | .5 |
| Forward Gain, dBi | 10.2 |
| Frequency, MHz | 144-148 |
| Front to Back Ratio, dB | 19 |
| Longest Element in(cm) | 40.75 (104) |
| Mast size range, in.(cm) | 1.25-2 (3.8-5.1) |
| No. Elements | 4 |
| Power Rating, Watts PEP | 2000 |
| Side Lobe Atten., dB, E-Plane | 40 |
| SWR 1.2:1 Typical 2:1 Bandwidth, MHz | 6 |
| Turning Radius ft(m) | 4 (1.22) |
| Weight, lb(kg) | 21.5 (9.75) |
| Wind load ft (m) sq | 4.84 (.45) |



Este producto sobrepasa 1 metro de longitud embalado. Serán añadidos 7€ de recargo adicionales de suplemento de transporte.