|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 124WB CUSHCRAFT |

|  |  |  |  |
| --- | --- | --- | --- |
| 127,00 €  |

|  |  |
| --- | --- |
|   | Add to baskethttp://www.radiocenter.es/contents/media/feedback_tick.png |

 |

 |

**144-148 MHZ 4 ELEMENTOS, GAIN 10,2DB.**

|  |  |
| --- | --- |
| Model  | 124WB  |
| 3dB Beamwidth, Degrees E-Plane  | 60  |
| 3dB Beamwidth, Degrees H-Plane  | 88  |
| Boom Lenght ft.(m)  | 4(1.22)  |
| Electrical Wavelength  | .5  |
| Forward Gain, dBi  | 10.2  |
| Frequency, MHz  | 144-148  |
| Front to Back Ratio, dB  | 19  |
| Longest Element in(cm)  | 40.75 (104)  |
| Mast size range, in.(cm)  | 1.25-2 (3.8-5.1)  |
| No. Elements  | 4  |
| Power Rating, Watts PEP  | 2000  |
| Side Lobe Atten., dB, E-Plane  | 40  |
| SWR 1.2:1 Typical 2:1 Bandwidth, MHz  | 6  |
| Turning Radius ft(m)  | 4 (1.22)  |
| Weight, lb(kg)  | 21.5 (9.75)  |
| Wind load ft (m) sq  | 4.84 (.45)  |



Este producto sobrepasa 1 metro de longitud embalado. Serán añadidos 7€ de recargo adicionales de suplemento de transporte.